**BRCGS Food Safety Issue 8**

F806: Audit Duration Calculator

**Document Scope:** This document is applicable to all audits associated with Issue 8 of the Food Safety Standard. This document replaces all previous versions of the calculator including F806 Version 2 August 2018.

All audits starting on or after 1st April 2020 shall be completed in accordance with this version of the calculator. (Where audits have already been agreed with sites Issue 8 audits prior to this date may continue to operate to the previous duration calculator).

**Change log:**

|  |  |  |
| --- | --- | --- |
| **Version no.** | **Date** | **Description** |
| 1 | October 2016 | Updated for Issue 7:* Increase in audit duration by 2 hours in smaller sites
* Inclusion of requirement for actual time on site to be confirmed by the site and auditor for each day of the audit
* Recognition of the shorter percentage of time needed in the production facilities of small sites with simple operations
* Addition of information for the Global Markets Programme
 |
| 2 | August 2018 | Updated for Issue 8This version replaces previously published F701 (Audit Duration Calculator for Issue 7).The primary changes are:* Review of the duration requirements for the additional modules and Traded Goods Section of the Standard (Section 9)
* Addition of audit duration requirements for small sites
 |
| 3 | June 2019 | New BRCGS logo and footer changed |
| 4 | 08/10/2019 | Updated based on international feedback from certification bodies, frequently asked questions to BRCGS and the first 6 months of Issue 8 audits.N.B. This document excludes START! which is covered separately in the audit protocol for that programme. |

**1. Background**

Common practice is for BRCGS to review the auditor duration within 6 months of the launch of a new Standard to ensure that the values within the calculator remain appropriate for the change in requirements and auditing techniques within the new Issue. In completing this review and update BRCGS have considered international feedback from certification bodies, frequently asked questions to BRCGS and the first 4 months of Issue 8 audits.

In accordance with the calculator and current practice the typical audit duration shall be 18 hours of which approximately 9 hours (i.e. approximately half of the audit) shall be spent auditing the production environment, site facilities, interviewing staff and observing processes.

**2. Calculation of audit duration**

The audit duration calculator is based on:

* Number of employees – as full time equivalent employees per main shift including seasonal workers. This should be based on the maximum number expected in a shift.
* Size of the manufacturing facility (in square metres) - including onsite storage facilities. The conversion from square feet to metres is 10.76 (eg 86,000 square feet equals 8,000 square metres).
* The number of HACCP plans included within scope – for the purpose of this calculator, a HACCP plan corresponds to a family of products with similar hazards and similar production technology and will therefore usually correspond to the number of product types.

The other factors identified in the Standard (see appendix 1) may influence the calculation but are considered to be less significant. These other factors shall not influence the audit duration by more than 30% from the total calculated audit duration.

**Table of audit durations:**

When using the following table, it should be noted that a typical audit day is 8 to 10 hours (not including lunch breaks). Therefore an 18-hour audit could be completed as two 9-hour days, or alternatively as two 8-hour days with some additional time on the third day. An audit day must not exceed 10 hours, except in exceptional circumstances.

|  |  |
| --- | --- |
|  | **Audit duration based on 1 - 3 HACCP Plans (in days)** |
| **Size of manufacturing facility** |
| **No Employees** | **<10k sq. m** | **10k-25k sq. m** | **>25k sq. m** |
| 1 – 50 | 18 hours (Completed in 2 - 2.5 days) | 18 hours (Completed in 2 - 2.5 days) | 20 hours(Completed in 2 - 2.5 days) |
| 51 – 500 | 20 hours (Completed in 2 - 2.5 days) | 24 hours (Completed in 2.5 - 3 days) | 26 hours (Completed in 3 - 3.5 days) |
| 501 – 1500 | 22 hours (Completed in 2.5 - 3 days) | 26 hours(Completed in 3 - 3.5 days) | 30 hours (Completed in 3.5 - 4 days) |
| >1501 | 22 hours (Completed in 2.5 - 3 days) | 32 hours(Completed in 3.5 - 4 days) | 34 hours(Completed in 4 - 4.5 days) |

Where a site is exceptionally small, a shorter audit duration may be applicable. In this situation the site must meet all of the following criteria:

• There is only one, simple production process (for example, a small produce pack house, packing whole, fresh produce)

• The main shift consists of 5 or less employees

• The size of the manufacturing facility is 5k sq. m or less

In these circumstances an audit duration of 12 hours may be applied. As mentioned below, the auditor may identify reasons for an adjustment in the audit duration (for example for a well prepared or poorly prepared site), but under no circumstances shall the audit duration be less than 8 hours.

**Additional time allocation**

There are several situations which require time to be added to the audit duration tabulated above. These are where a site has:

* more than 3 HACCP plans
* high risk, high care or ambient high care products and needs to be audited against Section 8 of the Standard
* traded products audited to Section 9 of the Standard
* an audit including one or more additional modules
* inclusion of the Ethical Trade & Responsible Sourcing (ETRS) risk assessment

|  |  |
| --- | --- |
| **Additional HACCP Plans** | **Additional time (This time to be split between document review and the production environment)** |
| 4 – 6 plans | 4 hours (0.5 day) |
| 7 or more plans | 8 hours (1 day) |

|  |  |
| --- | --- |
| **Additional sections of the Standard** | **Additional time****(This time to be split between document review and the production environment)** |
| Section 8 (High Risk, High Care or Ambient High Care) | 2 hours per area |
| Section 9 (Traded Products) | ≥1 hour |

|  |  |  |
| --- | --- | --- |
| **Additional module number** | **Module title** | **Typical additional time required** |
| 10 | GlobalG.A.P. Chain of Custody | ≥1 hour |
| 11 | Meat Supply Chain Assurance | 2 - 4 hours (0.25 - 0.5 day) |
| 12 | AOECS Module for Gluten-Free Foods | 2 - 4 hours (0.25 - 0.5 day) |
| 13 | FSMA Preventive Controls Preparedness | 2 - 4 hours (0.25 - 0.5 day) |

|  |  |
| --- | --- |
| **Additional activity** | **Typical additional time required** |
| Ethical Trade & Responsible Sourcing (ETRS) Risk Assessment | 4 hours (0.5 day) |

**2.1 Time spent within the production environment**

The audit of a site to the Standard will involve time spent both within the production environment and reviewing records and procedures within an office.

Wherever practicable, evidence should be gathered within the production environment through interviewing staff, observing working practices and reviewing process controls and records.

Therefore, for a majority of sites, approximately 50% of the audit will be spent auditing production and site facilities, interviewing staff, observing processes and reviewing documentation in production areas with the relevant staff. However, it is recognised, that in smaller, simple operations, the time required may be less than 50% of the audit. In these circumstances the amount of time spent in production and site facilities can be reduced, but the expectation is that at least 30% of the audit (e.g. 0.5 day minimum for a 1.5 day audit), will still be spent in these areas. Where the size of the site is larger than 50 employees and 10,000 square metres then an increased proportion of the time allocated to the audit will be spent within these areas.

The production environment includes external site inspections as well as visits to ancillary services, for example maintenance departments, laboratories, NPD and despatch departments. Good practice is for the auditor to make multiple visits into the production areas to view different activities, processes, areas of the facility or shifts, rather than spending one day (or one block of time) in production and one reviewing paperwork.

The duration of the audit of production and site facilities must be recorded in man hours (using whole numbers e.g. 6 not 5.5) giving the total time that has been spent in these areas. Any deviation from the calculated audit duration (either for total audit duration or for the time spent in production and site facilities) needs a valid justification which is recorded on the audit report.

Multiple identical key processes, such as several identical packaging machines, need not extend audit duration as sampling during the audit should address those identical functions. However, where there are significant variations or the auditor has concerns that require additional investigation (e.g. auditing of additional examples of the process) additional time shall be allocated.

**3 Total time calculation**

A typical audit day shall be 8 hours (not including lunch breaks) and should not exceed 10 hours, except where there are exceptional circumstances.

On-site audit duration should be stated in total man hours (using whole numbers e.g. 17 not 16.5) giving the time at the site conducting the audit (including time in production).

The start and finish times each day shall be clearly stated on the audit report and reflect the actual times at the site. These should be agreed as correct between the auditor and the authorised site representative i.e. the site should sign a record of the start and finish times, for each day of the audit, a copy of which must be retained by the certification body. (This may be combined with other audit documentation, for example, by adding the information to the non-conformity record sheet).

Allowance should be made (to deduct time) where audit teams are used and both auditors are present e.g. at the opening and closing meetings. Those personnel not ‘auditing independently’ should not be included within the total time calculation e.g.:

* Witness auditor
* Trainee auditor
* Technical expert

Where a combination of audits has been undertaken e.g. BRCGS and ISO22000, then a calculation for the total time taken for the Global Standard audit only should be stated. BRCGS expect that additional time is allocated over and above the minimum time for the Global Standards audit whenever a combination audit is undertaken.

The total hours shall not include any calculation for writing of the final audit report away from site. This is additional time and is typically 4 – 8 hours.

**Appendix 1**

Factors which may influence the duration of the audit are:

* initial audit (i.e. the site’s first ever audit) – it is likely that the auditor will require additional time, for example, during opening and closing meetings.
* complexity of the manufacturing process
* number of product lines – for example, this could mean there are a larger number of potential hazards (e.g. a large number of allergens onsite), making HACCAP review or auditing of control mechanisms longer than typical.
* size and age of site and impact on material flow
* labour-intensity of processes
* communication difficulties, e.g. language
* the number of non-conformities recorded in the previous audit – clause 1.1.12 requires the site to complete root cause analysis and preventive recurrence of non-conformities identified at the previous audit. Therefore, a large number of non-conformities at the last audit are likely to require increased time for the auditor to assess.
* difficulties experienced during the audit requiring further investigation
* the quality of company preparation, e.g. documentation, HACCP, QMS
* additional storage facilities, locations or head office assessments included within the audit process
* a separate audit of the central system (head office audit) completed before the manufacturing site audit may reduce the duration calculated for the manufacturing site audit to take account of systems already audited at the central (head) office. This is typically a reduction of 2 hours.